Here are a few tips for working with these templates:

-Each template is true to scale and for a specific switch (unlike the Outline Drawings which may cover multiple sizes and may not be to scale).

-Each view within each template is saved as a block.  Typically each drawing has a front view and a side view, but some drawings may have additional views or sections.  If you insert our template drawing into your own drawing, you probably want to explode it once, but only once.  That way each view can be moved as single object to locate as you desire.

-We have tried to keep our templates as clean and simple as possible.  Other than the base layer “0”, we have keep the number of layers used to a minimum and all the layer names start with “B-“ so they stay grouped together in your layer commands.  Depending on your situation, you may wish to turn off the construction layer “B-CONSTR” when you print and adjust other line weights that are determined by layers as necessary.  Also, to keep the drawing files as small as possible, we have tried to purge all unnecessary blocks, styles, layers, etc.

-All template drawings are 2D.